**CRS**

Security system

|  |  |
| --- | --- |
|  | **REQ\_CRS\_ID\_1** |
| **Description** | The safe opens using a 4 character password which is displayed on a LCD and a message representing the password status is displayed (success or wrong). |

|  |  |
| --- | --- |
|  | **REQ\_CRS\_ID\_2** |
| **Description** | A LED should blink if the password is entered wrong 3 successive times. |